from gpiozero import LED

from time import sleep

from gpiozero import LED

from time import SLEEP

red = LED (22)

amber = LED (27)

green = LED (17)

red . blink (1, 1)

amber . blink (2, 2)

green . blink (3, 3)

red = LED (22)

amber = LED (27)

green = LED (17)

red. on ( )

sleep (1)

amber . on ( )

sleep (1)

green . on ( )

sleep (1)

red. on ( )

sleep (1)

amber . on ( )

sleep(1)

green . on ( )

sleep (1)

red. off ( )

sleep (1)

amber . off ( )

sleep(1)

green . off ( )

while True:

red. on ( )

sleep(1)

amber . on ( )

sleep (1)

green . on ( )

sleep (1)

red. off ( )

sleep (1)

amber . off ( )

sleep (1)

green . off ( )